KariAnn Harjo

ITSE 1450

Module 10 Discussion 4

BSS and ESS differ mainly in terms of scale and connectivity. A BSS is a basic, standalone Wi-Fi network, functioning with a single access point, suitable for limited areas like a single office or home. ESS, on the other hand, is essentially a network of multiple BSSs, allowing for extended coverage and mobility. In an ESS, users can move between different BSSs (or APs) without losing connection, making it ideal for larger spaces that require continuous wireless coverage over multiple access points.